Tecanno air vent Frame 100, brushed stainless steel, for supply and exhaust air in design-type construction (0033100-9005-20).

For installation on ceilings and walls via 100 mm connecting pieces. 100 percent freely usable cross section. Can be comined with volume flow regulator or filter insert from Tecanno. The flush cover ensures a consistently slim design with a symmetrical, flow-optimized air throughput. Front made of brushed stainless steel; blase plate made of sheet steel with electrostatic powder coating (RAL 9005-20). Made in Germany. Registered design patent.

Dimensions: L x W x H (mm): 220 x 220 x 14

Nominal size: 100 mm
Volume flow range: 10-37 m³/h

Manufacturer: Tecanno
Type: Vent Frame 100, brushed stainless steel
Item No.: 0033100-9005-20