Tecanno air vent Five 100 for supply and exhaust air in design-type construction (0005100-9016-20).

For installation on ceilings and walls via 100 mm connecting pieces. 100 percent freely usable cross section. Can be combined with volume flow regulator or filter insert from Tecanno. The flush cover ensures a consistently slim design with a symmetrical, flow-optimised air throughput. Vent made of sheet steel with electrostatic powder coating (RAL 9016-20). Made in Germany. Registered design patent.

Dimensions L x W x H (mm): 260 x 260 x 10

Nominal size: 100 mm
Volume flow range: 10-37 m³/h

Manufacturer: Tecanno
Type: Ventil Five 100
Item No.: 0005100-9016-20