Tecanno air vent One 125 for supply and exhaust air in design-type construction (0001125-9016-20).

For installation on ceilings and walls via 125 mm connecting pieces. 100 percent freely usable cross section. Can be combined with volume flow regulator or filter insert from Tecanno. The flush cover ensures a consistently slim design with a symmetrical, flow-optimized air throughput. Vent made of sheet steel with electrostatic powder coating (RAL 9016-20). Made in Germany. Registered design patent.

Dimensions (LxWxH): 224 x 224 x 12 mm  
Nominal size: 125 mm  
Volume flow range: 10-54 m³/h

Manufacturer: Tecanno  
Type: Vent One 125  
Item No.: 0001125-9016-20