Tecanno air vent One Plus 160 for supply and exhaust air in design-type construction (0101160-9016-20).

For installation in ceilings and walls via 160 mm connecting pieces. 100 percent freely usable cross section. The flush cover ensures a consistently slim design with a symmetrical, flow-optimized air throughput. Vent made of sheet steel with electrostatic powder coating (RAL 9016-20). Made in Germany. Registered design patent.

Dimensions L x W x H (mm): 256 x 256 x 40

Nominal size: 160 mm  
Volume flow range: 10-175 m³/h

Manufacturer: Tecanno  
Type: Vent One Plus 160  
Item No.: 0101160-9016-20